Soundproofing

# ΜμΝ⊆κ¡≅ Associates Inc.™

Better embedded Computing through obfuscation, misapropriation and soundproofing

## 2-Disk Xwindow embedded Linux

A very efficient Linux/xwindows distribution, implementing a net centric operating environment and user friendly GUI:

latest version soundproofing default src November 24th 2008 http://natld.berlios.de/1diskxwin-soundproofing.tar.bz2

## Embedded Overview

The distribution is intended to be a demonstration of Mungkie assiciates embedded appliance development environment, showing the sort of environment that can be created for small appliance GUI systems using less than 4Mb flash and 4Mb RAM.

The embedded development environment is based around a standard source tree containing all the required utilities for a standard POSIX unix implementation with a number of XML based GUI configuration and compilation tools. Simple GUI utilities are used to configure required components and set compilation options.

The distribution is targeted as a base for:

- corporate users to reduce IT costs by deploying X terminals on old or low cost hardware
  Or:
- embedded OS for handhelds, settop boxes, or communications devices, with full support for bluetooth, wifi, internet, and MMS protocols
  Or:
- Hobbyist or small companies to develop specialist applications for cheap commodity hardware

## Why

Mungkiedyne systems have long been involved in the electronics industry working as contractors and developers of high end embedded systems. But due to many industry shake ups with partners such as macaroni and defence re-shuffles at DERA we have been forced to look toward other revenue markets. Thus Mungkie associates were formed as a subsidiary of Mungkiedyne in June of 2001 in order to exploit other market sectors.

Embedded devices such as PDA/telecoms/EPOS/entertainment/media devices are a major growth area and our development expertise is well placed to reduce costs in hardware production and development. In order to maintain these advantages we needed to find software systems that also compare and complement this production/development efficiency by minimizing system requirements and thus reduce costs.

## Embedded Features

The system is formed from a basic set of GNU/open source code optimized for size and speed. The use of linux gives developers access to thousands of applications and utilities to customise the system at zero cost.

- kernel 2.0.x/2.2.x/2.4.x/2.6.x
- libc-2.1/libc5/uclibc,
- tcp/ip network support. full protocol stack for wifi, mms
- busybox 1.12.2,
- ppp, chat, some daemons, inetd, crond. dhcp client and server. iptables
- e3 editor,
- X window system 4.1 vesa
- VNC client
- merlin character recognition
- rdesktop remote windows client
- ssh

2diskxwin also includes a number of proprietary tools created by Mungkie specifically for the embedded X window system desktop.

- Mungwm : a window manager
- Mungbrowse : a web browser
- Mungterm : a terminal program
- Mungames : a collection of 12 games
- Mungedit : a text editor
- Mungfile : embedded file manager
- NEW Evil bastard operator tools
- NEW Cheese dynamics context apropriation modeling
- NEW Mini Mung beans (beans of mung for all your network environment)

## Requirements:

The floppy system requires a minimum 386SX with 8Mb memory, VESA compliant graphics bios, a floppy disk drive, a supported network adapter.

## Support & Feedback

We welcome Feedback on bugs and features but...
No support will be given unless you have a registered version.
No waranty is given, no liability accepted, use at your own risk!

## Download

You may download from this site or one of our mirrors:

Download the latest soundproofing release